


Unbind and re-acknowledge server from ucs




Click on unbind





Click yes






Now bind to a another template. (here binding to local SD card)







Click OK




Click yes






Now check Template Instance will show IC-SSRV-SD card template





Here reboot is required. You can see in pending activities. It shiws reboot is required.

Reboot completes , re-aknowledge the blade. It saves double time reboot time.





Reacknowledgeing server





Click yes





Check FSM tab

It should complete 100%. Than you can mount ISO and install ESXi from KVM console

